ABPmer Notice to Mariners: 
Survey Instrument – Seabed Deployment	
Introduction
APEM Group Ltd has commissioned ABPmer to undertake a monitoring programme within the transitional and coastal (TraC) waters of the River Roach, River Blackwater and River Colne.  

As part of this programme, ABPmer will be deploying CTD instruments (to observe temperature and conductivity/salinity) at five locations in these rivers for a 30-day period. The deployments are planned to take place on approximately 13-15 October 2026 and will be recovered approximately 30 days later.

During deployment/recovery operations, the vessel Jean T will be on respective locations for an approximate 1-hour period. When stationary other vessels are requested to pass at a safe speed and distance. VHF Channels 11 and 16 will be monitored throughout survey operations.

Mooring Details
The monitoring instruments will be secured within a seabed frame which will protrude above the seabed by 0.5 m in water depths ranging between 0m and 3.0m below Chart Datum. The frames will be secured to a 250kg sinker weight by weighted groundline. From the weighted groundline will be a riser chain to a surface marker buoy, a yellow special mark exhibiting light characteristics Y.Fl(5)20s.
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Figure 1.	Surface marker buoy
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Location Details
[bookmark: _Ref227326035]Table 1.	Seabed deployment locations
	Known Locations
	ETRS89
	OSGB36 (OSTN15)
	Water depth (mCD)

	
	Latitude
	Longitude
	Easting
	Northing
	

	Colne - BCCTS1 - River
	51° 51.00880' N
	0° 58.00884' E
	604432
	220999
	0.5

	Colne - BCCTS2 - Estuary
	51° 48.28371' N
	1° 0.21486' E
	607172
	216053
	3.0

	Blackwater - BCCTS3 - River
	51° 43.36970' N
	0° 47.70971' E
	593155
	206375
	3.0

	Blackwater - BCCTS4 - River
	51° 43.70214' N
	0° 43.94684' E
	588801
	206827
	0.0

	Crouch/Roach - BCCTS7 - River
	51° 35.12602' N
	0° 47.99322' E
	594067
	191111
	3.0
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Figure 2. 	River Crouch/Roach location (1)
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Figure 3. 	River Blackwater locations (2)
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Figure 4. 	River Colne locations (2)

Survey Programme
The following table sets out the anticipated survey deployment programme, progress and weather permitting.

Table 2.	Anticipated Deployment Programme
	Date
	Activity

	13-15/10/2026
	Seabed frames and surface marker buoys deployed using vessel Jean T

	-
	Frames and surface marker buoys remains on location for deployment period. Buoy is yellow special marked with light characteristics Y.Fl(5)20s.

	w/c 16/11/2026
	Seabed frames and surface marker buoys recovered using vessel Jean T


Vessel Details
Deployment/recovery operations will be undertaken from the Jean T. When stationary (during deployment/recovery) other vessels are requested to pass at a safe speed and distance. VHF Channels 16 and 11 will be monitored throughout survey operations.

Table 3.	Vessel Details
	Vessel
	Description

	[image: ]
	Jean T

Owned and operated by Portflair Ltd
Bradwell-on-Sea

LOA: 16.9 m
Beam: 5.2 m
Call Sign: MVS06
MMSI No: 235081274
VHF: 16 & 11


Contact Details
ABPmer management contact details are available in the table below.

Table 4.	Project Contacts
	Name 
	Organisation
	Contact Number
	Contact Email

	Paul Clement
Project Manager
	ABPmer
	07850 500315
	paul.clement@abpmer.co.uk

	Tom Wilson
On-board Surveyor
	ABPmer
	07708 396967
	twilson@abpmer.co.uk

	General Office
	ABPmer
	02380 711840
	



image3.png
ol .
P
- H





image4.png
=
AN

%

rw\m\umgw spit

Sevage VoAl S
e

JSLAND

Moorias

5
o wwes )
Mundor





image5.png




image6.png




image1.png




image2.jpg




